**Update Manual Through U Disk**

**- only for update from 1.2.X to 1.3.X**

**Update manual through USB Drive （only for from 1.2.X to 1.3.X）**

1、If the version is 1.2.X and below (such as 1.1.0, etc.), the update to 1.3.X version through U disk requires four files:

appfs\_special\_hi3536;

firmware3536;

N0I\_UI1B\_133.fls;

ubt3536m.

Put the four files into the USB flash drive. Plug the U Disk to the USB port of the N9000 device, then power off the N9000 device to automatically upgrade.




Figure 1 Update files required


During the upgrade process, the system will be prompted to upgrade (**Figure 2**). In about 5 minutes, the first step of update will be successful as shown like **Figure 3** and **Figure 4**. 

Figure 2




Figure 3




Figure 4

2、The device then automatically upgrades to version 1.3.3 (no need to remove the USB flash drive and reboot), the device screen will display the system prompts for upgrade (**Figure 5**). The boot logo will appear in about 2 minutes, and it will last for about half a minute. Then there will be an upgrade progressing bar (**Figure 6**), and it takes about 2 minutes to enter the system. At last, the upgrade is complete.




Figure 5




Figure 6 Update processing bar

**Note**：If the U Disk is connected to the device and the device is powered off for a period of time, the screen is always black. You can try to plug in the video cable. If it is still black, you can unplug the U disk or try another USB port.